[UniVBIOS v1.060401]
[UniVBIOS v1.00.00]
[UniVBIOS v1.00.00]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.53]
1. Feature Modify: Support DDRII in XG21
2. Feature Modify: Fixed about VESA function 15h failed.
[FlashRom V1.15.42 10/28/05]
1. bug fix: Dos flash version match up win flash.
    Fix chip info error in win flash. 

[FlashRom V1.15.41 12/08/04]
1. bug fix : BIOS version difference when use flash 1

[FlashRom V1.15.40 12/06/04]
1. bug fix : checksum only 75%
2. feature modify: modify code for search from bus 0-255

[FlashRom V1.15.39 11/12/04]
1. support multiple adapter PCI + PCI

[FlashRom V1.15.36 07/30/04]
1. bug fix:XG20  #20 

[FlashRom V1.15.36 07/30/04]
1. bug fix:XG20  #20 

[FlashRom V1.15.35 07/14/04]
1. feature modify: modify code for XG20 flash address

[FlashRom V1.15.34 07/12/04]
1. feature modify: modify code for XG20 32k decode size

[FlashRom V1.15.32 06/28/04]
1. feature add: support XG20

[FlashRom V1.15.31 06/09/04]
1. feature modify: change DRAM definition
2. feature add: add DRAM type: SamsungF Tsop

[FlashRom V1.15.30 06/04/04]
1. feature add: add DRAM type: AData Tsop, Nanya Tsop,Elixir Tsop

[FlashRom V1.15.29 06/01/04]
1. feature modify: change name from Mira to Kreton
2. feature modify: modify code for secondary adapter judgement
3. feature modify: refine code for GetROMInfo

[FlashRom V1.15.26 04/22/04]
1. feature modify: DRAM information change for Mira Tsop

[FlashRom V1.15.23 04/07/04]
1. feature add:Add interface for Utility to check rom file information
2. feature modify:modify interface for utility to get rom information

[FlashRom V1.15.22 03/24/04]
1. feature modify:SectorErase, wait blank time, change to 20 sec. for MXIC MX29F001T
2. feature modify:refine code for GetRomInfo(), refine function call for GetRomFileInfo,ValidateVBIOSRom

[FlashRom V1.15.21 03/24/04]
1. feature add:Support XG45

[FlashRom V1.15.20 03/18/04]
1. feature modify:change read vbios version position
2. feature add:add ValidateVBIOSRom function

[FlashRom V1.15.19 03/5/04]
1. feature add:add new SPI ROM chip support
   SPANSION S25FL001D, S25FLK05D
   ST: M25P05-A
   
[FlashRom V1.15.18 02/24/04]
1. feature modify:add bus 3 ,vga card check
2. feature add:add DRAM, VBios version

[FlashRom V1.15.17 02/17/04]
1. feature add: Add new PARALLEL ROM support: ST M29W010B

[FlashRom V1.15.16 01/15/04]
1. feature add:Add new SPI ROM support
   ST: 25P05V6
   ATMEL: AT25F512N
   PMC: 25LV512
   SAIFUN: SA25C1024

[FlashRom V1.15.15 12/25/03]
1. bug fix:fix V1.15.14 flash bug
2. bug fix:fix hang when SPI flash used in the second time

[FlashRom V1.15.14 12/19/03]
1. bug fix:fix AGP+PCI for SPI ROM, flash failure

[FlashRom V1.15.13 11/14/03]
1. bug fix:change vbios reserve area to 512 byte

[FlashRom V1.15.12 10/28/03]
1. feature modify:Add SST25VF512 SPI ROM
2. feature add:Add NFlash.exe

[FlashRom V1.15.11 ]
1. feature add:Add GetVGAChipDetailID
2. feature add:Add Device ID 40, Vendor ID 18CA
3. feature add:Add SPI check

[FlashRom V1.15.10 ]
1. feature add:Add new usage for XG40.
2. feature modify:remove SiS Logo
3. feature modify:change exe file name
4. feature add:add GetVGAType new interface for Windows 9x AP
5. feature modify:change 0x34018CA to 0x4018CA

[FlashRom V1.15 ]
1. feature add:Add multi-adapter flash for XG40.

[FlashRom V1.14 ]
1. feature modify:Modify SPI flash for DOS 

[FlashRom V1.13 ]
1. feature modify:Modify ICE29LF512 unprotect
2. feature modify:Modify PM39LV512 and PM39lv010

[FlashRom V1.12 ]
1. feature add:Support SPI flash for DOS 

[FlashRom V1.11 ]
1. feature modify:Support VB display
2. feature add:Support ICE29LF512 

[FlashRom V1.10 ]
1. feature add:Support new rom file of Xabre600 

[FlashRom V1.08 ]
1. feature add:Support Win98 flash
2. feature add:Can Backup rom file (ex:flash 4 backup.rom) 

[FlashRom V1.07 ]
1. feature modify:Add PCI Bus 2

[FlashRom V1.06 ]
1. feature add:Add new type include W39F010,W39L010,W39L512




[WinFlash V1.15.42 10/28/05]
1.bug fix : Z9 chip info show error.

[FlashRom V1.15.41 12/08/04]
1. bug fix : BIOS version difference when use flash 1

[FlashRom V1.15.40 12/06/04]
1. bug fix : checksum only 75%
2. feature modify: modify code for search from bus 0-255

[WinFlash V1.15.37 08/24/04]
1. feature modify: Search XGI from bus no. 255


[WinFlash V1.15.35 08/24/04]
1. feature modify: CheckSum code refine, maximum check size : 64k

[WinFlash V1.15.34 07/12/04]
1. feature modify: modify codes of IOCTL_SIS_LIB_SELECTFLASHRANGE for XG20

[WinFlash V1.15.33 07/09/04]
1. bug fix: XG4X #1884

[WinFlash V1.15.32 06/29/04]
1. feature add: add XG20 support

[WinFlash V1.15.31 06/09/04]
1. feature modify: change DRAM type definition
2. feature add: add DRAM type: SamsungF Tsop

[WinFlash V1.15.30 06/04/04]
1. feature add: add DRAM type: AData Tsop, Nanya Tsop,Elixir Tsop

[WinFlash V1.15.29 05/31/04]
1. feature modify: change name of DRAM_Type 8 to Kreton
2. bug fix: fix bug Pre-Test #483
3. feature modify: check rom deocde size when erase

[WinFlash V1.15.28 05/26/04]
1. bug fix: fix bug Pre-Test #483

[WinFlash V1.15.27 04/22/04]
1. bug fix: fix bug #1839

[WinFlash V1.15.26 04/22/04]
1. feature modify: GetDRAMType change for Mira Tsop

[WinFlash V1.15.25 04/15/04]
1. feature add:support multiple adapter flash

[WinFlash V1.15.24 04/13/04]
1. feature modify:rebuild sys

[WinFlash V1.15.23 04/07/04]
1. feature modify:Modify SELECTFLASHRANGE interface

[WinFlash V1.15.22 04/05/04]
1. feature modify:refine codes of wflash.c, for GetPart1Port(), GetExtIOBase()
2. bug fix:Fix bug# 1741
3. feature modify:Modify SELECTFLASHRANGE interface

[WinFlash V1.15.21 03/24/04]
1. feature modify:change SectorErase , MXICErease wait blank time for MXIC MX29F001T
2. feature add:add SELECTFLASHRANGE interface
3. feature add:Support XG45

[WinFlash V1.15.20 03/18/04]
1. feature add:add new SPI ROM chip support
   SPANSION S25FL001D, S25FLK05D
   ST: M25P05-A
   
2. feature add:add DRAM, VBios version interface
3. feature add:add ValidateVBIOSRom interface
4. feature add:support AMD64bit

[WinFlash V1.15.17 02/16/04]
1. feature add:Add new PARALLEL ROM:ST M29W010B support

[WinFlash V1.15.16 01/15/04]
1. feature add:Add new SPI ROM support
   ST: 25P05V6
   ATMEL: AT25F512N
   PMC: 25LV512
   SAIFUN: SA25C1024

[WinFlash V1.15.15 12/25/03]
1. bug fix:fix hang when SPI flashed in the second time

[WinFlash V1.15.13 11/14/03]
1. feature modify:vbios reserve area change to 512 byte 

[WinFlash V1.15.12 10/28/03]
1. feature add:Add SST25VF512 SPI ROM 

[WinFlash V1.15.11 09/10/03]
1. feature add:Add SPI interface
2. feature add:Add device Id 40 Vendor Id 18CA
3. feature add:Add GetVGAChipDetailID()

[WinFlash V1.15.10 09/01/03]
1. feature add:support XG40

[WinFlash V.1.11 12/05/02]
1. feature add:Support VB display
2. feature add:Support ICE 29LF512

[WinFlash V.1.10 11/22/02]
1. feature add:Support for Win9x
2. feature add:Multi-language Support
3. feature add:Support for Xabre 600
4. feature add:Support SST 39VF512


[WinFlash V.1.01 09/30/02]
1. feature add:Add for Customized (sisflash.ini)

[WinFlash V.1.00 09/19/02]
1. Fisrt release for WinFlash (Win2K/WinXP only)


[ManuTest 0.60.00]
1. Feature Add (VBIOS) : Support XG20.
2. Feature Add (VBIOS) : Add Dram address pin test.

[ManuTest 0.70.00]
1. Feature Modify (VBIOS) : No support macro vision,
2. Feature Modify (VBIOS) : Modify dram address pin test.
3. Feature Modify (VBIOS) : 2D test reback the original name 2DXG40.EXE in XG20.

[ManuTest 0.80.00]
1. Feature Add (VBIOS) : Support DRAM stability test in XG20.
2. Feature Modify (VBIOS) : Modify Bisttest.exe and modify ECLK source. 

[ManuTest 0.90.00]
1. Feature Modify (VBIOS) : Fix XG42 product display incorrect.

[ManuTest 1.01.07]
1. Feature Modify (VBIOS) : Fix PCI address search error in Intel integrated chip MB.

[ManuTest 1.01.08]
1. Feature Modify (VBIOS) : Modify the DRAMType (DDR2x->DDR) in manutest.inf	

[ManuTest 1.01.09]
1. Bug Fix (VBIOS) : Fixed dram test aborted in XG20.

[ManuTest 1.01.10]
1. Bug Fix (VBIOS) : Error message on screen after run XG20 SLT. 

[ManuTest 1.01.11]
1. Bug Fix (VBIOS) : Fixed return code error in SLT.

[ManuTest 1.01.12]
1. Bug Fix (VBIOS) : Fixed multi adapter failed in SLT.
2. Feature add (VBIOS ) : Add options for output filename, loop ocunt, and script infname.  

[ManuTest 1.02.00]
1. Feature add (VBIOS ) : New SLT Request to collect the log file into main log.  

[ManuTest 1.02.01]
1. Bug Fix (VBIOS ) : fixed 2dtest fail in xg20.

[ManuTest 1.02.02]
1. Bug Fix (VBIOS) : modify bisttest use gnu to fix dos32 page fault under 2g or 4g system memory with himem.sys.  

[ManuTest 1.02.03]
1. Bug Fix (VBIOS) : modify Run SLT S1.02.02B loop fail (testdram fail)

[ManuTest 1.02.04]
1. Bug Fix (VBIOS) : fix Run stability fail, allocmemory fail

[ManuTest 1.02.05]
1. Bug Fix (VBIOS) : Fix dram failed message shown error in XG20 SLT. 

[ManuTest 1.05.00]
1. Feature Add(VBIOS) : Support XG21.

[ManuTest 1.05.01]
1. Feature Modify (VBIOS) : Modify chip info in XG21 SLT.

[ManuTest 1.05.02]
1. Bug Fix (VBIOS) : Fix ECLK data error.

[ManuTest 1.05.03]
1. Bug Fix(VBIOS) : Fix Cfg info show random fail.

[ManuTest 1.05.04]
1. Bug Fix(VBIOS) : After disable CRB4[1], must delay some time to get CR48.

[ManuTest 1.05.05]
1. Bug Fix(VBIOS) : Show correct MCLK in DDRII XG21.
[UniVBIOS v1.060401]
[UniVBIOS v1.00.00]
[UniVBIOS v1.00.00]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.52]
[UniVBIOS v1.05.53]
1. Feature Modify: Support DDRII in XG21
2. Feature Modify: Fixed about VESA function 15h failed.
