;===============================================================================
; AST1100/1300/1400/2000/2050/2150/2100/2200/2300/2400 VBIOS ReadMe
;===============================================================================
1.Update VBIOS Image under DOS
- flash [updated image file] [old image file]
2.VBIOS Directory Descriptions:
- AST2000: for AST2000
- AST2000.D5: for AST2000 Display Banner last for 5 sec
- AST1100: for AST1100
- AST1100.D5: for AST1100 Display Banner last for 5 sec
- AST2050: for AST2050
- AST2050.D5: for AST2050 Display Banner last for 5 sec
- AST2100: for AST2100
- AST2100.D5: for AST2100 Display Banner last for 5 sec
- AST2100.DVO: for AST2100 DVO support
- AST2150: for AST2150
- AST2150.D5: for AST2150 Display Banner last for 5 sec
- AST2200: for AST2200
- AST2200.D5: for AST2200 Display Banner last for 5 sec
- AST2300: for AST1300/2300
- AST2300.D5: for AST1300/2300 Display Banner last for 5 sec
- AST2300.DVO: for AST1300/2300 DVO Support
- AST2300.ITE: for AST1300/2300 + ITE66121 Support
- AST2400: for AST1400/2400
- AST2400.D5: for AST1400/2400 Display Banner last for 5 sec
- AST2400.DVO: for AST1400/2400 DVO Support
- AST2400.501: for AST1400/2400 + DP501 Support
3.VBIOS Image Descriptions for AST2100/2200:
- D2512x32.266: DDR2 512Mb(32Mx16) 2pcs 266MHz
- D21Gx32.266:  DDR2 1Gb(64Mx16) 2pcs 266MHz
4.VBIOS Image Descriptions for AST1100/2050:
- D21Gx16.200:  DDR2 1Gb(64Mx16) 1pcs 200MHz
- D2512x16.200: DDR2 512Mb(32Mx16) 1pcs 200MHz
- D1512x16.200: DDR  512Mb(32Mx16) 1pcs 200MHz
5.VBIOS Image Descriptions for AST2150:
- D21Gx16.266:  DDR2 1Gb(64Mx16) 1pcs 266MHz
- D2512x16.266: DDR2 512Mb(32Mx16) 1pcs 266MHz  
6.VBIOS Image Descriptions for AST1300/2300:
- ASTVBIOS.396:  MCLK = 396MHz
7.VBIOS Image Descriptions for AST1400/2400:
- ASTVBIOS.396:  MCLK = 396MHz
8.Contact Window:
- yc_chen@aspeedtech.com
- 886.3.578.9568 ext. 810
